{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["RT Config Form","Worksheet","Template Info","RealTime Channel Info","Board Serial Number Location"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RT Config Form","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Worksheet","index":1,"n_rows":100,"n_cols":6,"rows_kept":100,"cut":false,"hidden":false,"merged":[[1,1,1,6],[16,1,16,2],[16,3,16,4],[2,1,2,6],[14,2,14,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[4,1,4,3],[12,1,12,4],[10,2,10,6],[13,2,13,6],[15,2,15,6]]}
[]
[null,"AlarmAgent RealTime Configuration Worksheet"]
[]
[]
[null,"Contact Information"]
[null,"First Name:"]
[null,"Last Name:"]
[null,"Phone:"]
[null,"Email:"]
[null,"Company Name:"]
[null,"Account #:"]
[]
[null,"AlarmAgent Unit Information"]
[null,"RTU Name:"]
[null,"Customer Service ID:"]
[null,"Board Serial Number:"]
[null,"RealTime Configuration",null,"Template:",null,3]
[null,null,"Mode","Interval","Threshold","Sensitivity"]
[null,"Pump Combo 1"]
[null,"Pump Combo 2"]
[null,"Channel 3"]
[null,"Channel 4"]
[null,"Channel 5"]
[null,"Channel 6"]
[null,"Channel 7"]
[null,"Channel 8"]
[null,"Channel 9"]
[null,"Channel 10"]
[null,"Input Power"]
[]
[null,"AlarmAgent.Info Service:"]
[null,"Analog Reports per Day:"]
[null,"RealTime Event Channels:",0]
[null,"RealTime Sampling Channels:",0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"AlarmAgent"]
[null,"Raco Manufacturing Website"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[true]

{"sheet":"Template Info","index":2,"n_rows":78,"n_cols":2,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
[null,"AlarmAgent Template Information "]
[]
[null,"Template 1 : 2-Pump Duplex"]
[null,"Channel 1 - Pump Combo "]
[null,"Channel 2 - Pump Combo "]
[null,"Channel 3 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 4 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only "]
[]
[null,"Template 2 : 2-Pump with Flow Meter "]
[null,"Channel 1 - Pump Combo "]
[null,"Channel 2 - Pump Combo "]
[null,"Channel 3 - Totalizer "]
[null,"Channel 4 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only"]
[]
[null,"Template 3 : 3-Pump Triplex "]
[null,"Channel 1 - Pump Combo "]
[null,"Channel 2 - Pump Combo "]
[null,"Channel 3 - Pump Combo "]
[null,"Channel 4 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only"]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only "]
[]
[null,"Template 4 : 3-Pump with Flow Meter "]
[null,"Channel 1 - Pump Combo "]
[null,"Channel 2 - Pump Combo "]
[null,"Channel 3 - Pump Combo "]
[null,"Channel 4 - Totalizer "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only "]
[]
[]
[]
[]
[null,"Template 5 : Multi-purpose "]
[null,"Channel 1 - Normally Open, Normally Closed, or Status Only, Runtimer, or Totalizer "]
[null,"Channel 2 - Normally Open, Normally Closed, or Status Only, Runtimer, or Totalizer "]
[null,"Channel 3 - Normally Open, Normally Closed, or Status Only, Runtimer, or Totalizer "]
[null,"Channel 4 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only"]
[]
[]
[]
[null,"Template 7 : Multi-purpose "]
[null,"Channel 1 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 2 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 3 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 4 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 5 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 6 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 7 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 8 - Normally Open, Normally Closed, or Status Only "]
[null,"Channel 9 - Analog, Normally Open, Normally Closed, or Status Only "]
[null,"Channel 10 - Analog, Normally Open, Normally Closed, or Status Only"]

{"sheet":"RealTime Channel Info","index":3,"n_rows":22,"n_cols":1,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Real-Time Channel Configuration "]
[]
["MODE:"]
["v  Event: When a channel changes state for the length of the configured interval, the change information is transmitted in real time. Information includes the date, time, and state of the channel. Events are subject to throttling restrictions. Pump channels are allowed to transmit up to 288 events per day. Other channel types can report up to 100 events per day. "]
["v  Sampling: Channel data is transmitted on a configured schedule. Sample rate can be configured for a maximum of 1 sample per minute. Sampling is generally reserved for analog or power input channels."]
["v  Disabled: Real-Time features for this channel are disabled."]
[]
["INTERVAL: "]
["v  Event: The amount of time the channel must change state before the transition is considered an event. Minimum interval is 30 seconds. "]
["v  Sampling: The length of time between samples. Maximum sampling rate is one sample per minute."]
[]
["SENSITIVITY:"]
["v  Event: The percentage the data must change before the change is considered an event. For digital channels, the change is 100% so all digital events are delivered. For analog channels, this percentage change is configured as needed. Minimum sensitivity configuration is 10%."]
["v  Sampling: Sensitivity is ignored"]
[]
["THROTTLING: "]
["v  Event: The number of transitions allowed per day per channel. Pump channels are allowed 288 transitions per day. All other channels are allowed 100 transitions per day."]
["v  Sampling: Throttling is ignored."]
[]
["Important Note about the RTU Battery and Real-Time: If Real-Time is enabled, the Battery will report battery voltage every hour during a power failure. "]
[]
["Finding the Customer Service ID: The Customer Service ID for each RTU can be found on the \"Manage RTUs\" page in the AlarmAgent website. It can also be found on the printed \"RTU Information Sheet\" included with your unit."]

{"sheet":"Board Serial Number Location","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}