# Import RTU

To access the dialog box for this setting cancel the “Select RTU” dialog and select “Import RTU” from the top menu.

When the “Import RTU” dialog appears, use the browse window in the far left to find the Alarmware directory you would like to import the RTU from. When the directory is found, the middle window will display the available Catalyst configurations from the selected directory. Highlight the desired RTU(s) and click on the “Import” button. The configuration you selected should now appear in the far-right window or “Active RTU list.” When you close this dialog, the added RTU will appear in the “Select RTU” dialog.