# Front Panel LEDs

NORM | - ON when in NORMAL mode.
CHECK | - ON when in CHECK STATUS mode, local reports being delivered.
LOBAT | - ON when battery voltage falls below a threshold value. With fully charged battery, light should go OFF within a few minutes of turning ON. A discharged battery may take up to a day to fully recharge. If the battery is low and there is no power failure, the battery is CHARGING.
PFAIL | - ON during primary power failure and running on battery. During primary power failure, all LEDs will blink faster than normal. Upon return of power, all LEDs will stop blinking.
TFAIL | OFF if there is no unacknowledged TFAIL BLINK fast during unacknowledged TFAIL
NET 1 : PLC | OFF if scan is OFF ON if scan is ON BLINK if scan is ON and any channels on this net are in Communication ALARM (acknowledged or not)
NET 2 : PRINTER | ON when device is not flow-controlling the port BLINK if device is flow-controlling the port.
NET 3 : AWARE | OFF if no Alarmware™ session is active ON if Alarmware™ session is active BLINK if last outgoing session attempt failed to connect
PROGRAM | - ON when in PROGRAM mode via Front Panel, Over the Phone, or Alarmware™.
RECORDING | - ON when message is being recorded.
DISARMED | - BLINK when unit is disarmed.
PHONING | ON when off-hook for any reason SLOW BLINK during inter-session delay. Otherwise LED is OFF
LOGFILE | ON when the Log File is enabled OFF when the Log File is disabled SLOW BLINK when data has been lost
CHANNEL LEDs | BLINK when channel in ALARM state ON when alarm acknowledged - Regardless of when a channel is alarmed, the channel alarm LED will be in sync with all active channel alarm LEDs.

Note: Front panel LED representations in Alarmware™ should behave exactly as the Front Panel LEDs.