# Destination Settings -- Notification Reports

The Notification Report destination settings are available for, Telephone, Pager, Fax, and Remote Data Terminal.

Alarm Checkbox -- Check this box when you want to deliver a notification report to this destination when an alarm occurs. A telephone destination is the only destination type capable of acknowledging the report.

Alarm Acknowledgment Checkbox -- Check this box when you want to deliver an alarm acknowledged report to this destination when an alarm has been acknowledged.

Sort Report Contents By -- You have three ways to sort the notification report:

- Time the state tripped, first in, first out: Allows you to sort based on the time the alarm was tripped. This option will configure the Catalyst to report the alarms tripped first, then report each alarm until the last alarm tripped is reported.
- Time the state tripped, last in, first out: Allows you to sort based on the time the alarm was tripped. This option will configure the Catalyst to report the alarms tripped last, the report each alarm until the first alarm tripped is reported.
- Channel Number: Catalyst will sort the notification report so that lowest ordinal channel alarms are reported first.

Deliver Notifications – You have three type of notification delivery:

- Continually Until Acknowledged: Unacknowledged channel states are never considered as reported. Other channel states and log file items are considered reported as described under Until Reported option below. Hence, as long as there are any unacknowledged alarms, notification sessions are attempted and each report starts from the beginning.
- ALWAYS USE THIS RULE for destinations relied upon to provide alarm acknowledgment. This is the default rule for any destination type that has the ability to provide operator acknowledgment during the session (see table below).
- Only Once: All channel states as of the moment are considered reported at the moment the destination is contacted. Thus, no report will resume after initial contact and subsequent sessions happen only as new state changes or schedule events occur. Log file items are considered reported as described under Until Reported option below.
- NEVER USE THIS RULE if relying on the destination to archive data or to provide alarm acknowledgment. Rather, use only when partial reports are acceptable and session resumption is not desired. For examples:
  - Avoid exhausting a fax machine’s paper supply (at the risk of loosing report data) by setting the page limit to a small number and selecting this delivery rule. Reports will stop at that limit and not be resumed later on.
  - Allow factory floor personnel to stop a PBX report without complete delivery and without requiring acknowledgment of all alarms.
- `Until Reported: All channel states and log file segments are considered reported if and only if they are confirmed received by the destination. New sessions will take place, in rotation, only so long as there are unreported items. Reports will resume as required, and omit any data already reported. This rule guarantees that every event and channel state is reported and that those reports are not repeated.
- DO NOT USE THIS RULE when report repetition is desired. Any destinations fully relied upon to notify or correct alarm conditions should use the continually until acknowledged delivery rule. For example, there is no end-to-end confirmation of paging reports. This exposes any given report to loss (if the pager is turned off, for example). Hence, repetition is desirable for pager destination types.

The table below summarizes how the configured rule applies to each session/report type.

Session Type | Delivery Rule Used During Report
--- | ---
Alarm Notification | As configured on notification tab of destination dialog.
Acknowledgment Notification | As configured, except that continually until acknowledged is treated as until reported. (Because there is no way to acknowledge the acknowledgment report).
Test Callbacks | Always one attempt only, whether contact made or not.
Scheduled Test Calls | Always continually until acknowledged.
Status Reports | As configured on notification tab of destination dialog, except that "continually until acknowledged" will be treated as "until reported" (there is no way to acknowledge the status report).
Log File Reports | Always until reported. The log file segmentation granularity suffices, to prevent a lot of duplication when reports resume.

The table below summarizes the default delivery rule for destination type.

Destination Type | Default Delivery Rule (for alarm notifications)
--- | ---
Voice | continually until acknowledged
RDT | until reported
Alarmware | continually until acknowledged
Fax | until reported
RCS | continually until acknowledged
Numeric Pager | until reported
Alpha Pager | until reported
PBX | until reported