# Electrical Power Requirements

The product requires power input of one of the following:

- 120 VAC (nominal) 60Hz @ 70 mA maximum current
- DC power input of 8-16 VDC (12 VDC Nominal) input @ 900 mA maximum current
- 48 VDC +/- 10% @ 250 mA maximum current using an optional 48/12 VDC converter module
- 125 VDC +/- 10% @ 125 mA maximum using an optional 125/12 VDC converter module

The currents specified do not reflect initial momentary surge current, which can be several times the above figures.