# Session Parameters

The Session Parameters dialog box allows users to set:

- The number of redial attempts to reach a given Destination (if a busy signal is detected on the first try),
- The Session Inactivity timeout period after which the RTU will terminate a Front Panel, Over the Phone or Alarmware™ session if user interaction ceases
- The basis for reporting priority (lowest channel number versus lowest Destination number)
- The Inter-session Delay is the time delay between outgoing calls
- Microphone listening on/off. (provides for a 15 second listening period via the Catalyst's built-in microphone)
- The Menu Options Repeat parameter determines whether or not the menu options are to be repeated during an over the phone session. The options menu can be repeated up to 3 times.
- The Protocol Detection for Incoming Calls (S-Model Only) allows you to set the amount of time the Catalyst will wait to detect the protocol of an incoming call.

See Also

Redial Attempts

Session Time-Out

Inter-Session Delay

Microphone Listening Period