# Keycode Interpretation Table

OVER THE PHONE MENU OPTIONS | FEATURE (AS PIN ALLOWS)
--- | ---
1 | Acknowledge ALL alarms, enter PROGRAM mode
2 | Acknowledge ALL alarms, enter PROGRAM mode-Read Only
3 | Acknowledge ALL alarms, then report all Unreported and Non-Normal Channels not linked to Destination
4 | Enter SEARCH mode
5 | Repeat the Menu Options
6 | Repeat Unit ID message, Preliminary Report, and Alarm Report
7 | Mark ALL alarms as reported without acknowledgement
8 | Acknowledge ALL alarms, reported or unreported and give a count of the number of alarms
9 | Acknowledge ALL alarms, then report all Unreported and Unacknowledged Channels not linked to Destination
0 | Terminates the Session

ACTION | FROM THE FRONT PANEL | OVER THE PHONE
--- | --- | ---
Get STATUS report | Press the CHECK STATUS key | Keycode 00 in PROGRAM mode
Quit current Report or Mode | Press the CANCEL key | #**
Toggle arm/disarm state | Press the DISARM | RE-ARM key | Keycode *1 in PROGRAM mode
Go Off-hook, enter SPEAKER PHONE mode | Press the DIAL-OUT | PRESS TO TALK key | not available
Dial Number (SPEAKER PHONE mode only) | Phone String Characters (0 – 9, *, #) | not available
Talk (SPEAKER PHONE mode only) | Press the DIAL-OUT | PRESS TO TALK key | not available
Toggle Power | Press the POWER ON | OFF key | not available

The following are available when in PROGRAM or SEARCH mode:

ACTION | FRONT PANEL | OVER THE PHONE
--- | --- | ---
Insert Command digit | 0-9 | 0-9
Signal end of Command string | ENTER key | ###
Erase current command | CANCEL key | #**
Toggle recording state (prior command required to enable) | RECORD key | 0
Delimits command from set value (used to separate command fields) | * | *
Command value reset delimiter | ** | **
Sub-Sub-Field delimiter (e.g. routing nodes) | *** | ***
Shift the meaning of the following keystroke | # | #
Minus sign | ## | ##
Decimal point | #* | #*