# Telephone Line Connections

Plug a standard RJ11 telephone modular cable into the Telephone Jack located at the bottom end on the right hand side of the product. Plug the opposite end of this cable into an RJ11 telephone line service jack. This step may be skipped if the product has been ordered with the Cellularm™ Cellular option. In that case, refer to the separate instructions included with the Cellularm™ regarding establishing the necessary cellular telephone service.

Please refer to the FCC Notice to Users for details on FCC requirements for use of this product.