# Destination Settings -- Status Reports

Status Reports are available for OTP, Pager, FAX, and RDT destination types.

Include the destination in the "Autocall" roster -- Check this box if you want this destination to be included in the group of destinations that may be called when the Catalyst performs an Autocall. An Autocall is a test call made at scheduled intervals. See Conducting Test Autocalls.

Deliver Status Reports on the following schedule -- Check this box if you want the Catalyst to call this destination at scheduled intervals to deliver a Status Report.

- Base Time: Sets the time of day that the Catalyst will reference when determining when to deliver a report.
- Frequency: Determines how often the Status Report will be delivered to this destination.

Example: A base time of 00:00 and a frequency of 02:00 will result in scheduled reports sent to this destination at 00:00, 02:00, 04:00, 06:00, and so on, around the clock.

See Also

Status Reports