# Voice Mode Network ID Name Messages

The Voice Mode Network ID Name Message identifies the corresponding Industrial Network that is the source of most of the information in the report. In practical terms, this amounts to naming the PLC that the RTU is monitoring. The factory default Voice Mode Network ID Name Message for Net 1 is "Modbus Network".

Keycodes:

- To review all Voice Mode Network ID messages use Keycode 6 1
- To review the Voice Mode Network N ID message use Keycode 6 1 N
- To clear the Voice Mode Network N ID message to factory default use Keycode 6 1 N * *
- To record the Voice Mode Network N ID message use Keycode 6 1 N *