# Phone Configuration Keycodes

Keycode | Specification

Device Report
4 | Review complete device configuration report
4*N | Report entire configuration for Device N
4*N** | Restore all parameters for Device N to default
4*N*0 | Enable Scan on Device N
4*N*1 | Disable Scan on Device N

Telephone Device Report
40 | Review all telephone configuration items
40** | Reset all telephone configuration items to default

Call Progress Monitoring
401 | Read status of Call Progress Monitoring (CPM)
401** | Reset CPM to default
401*0 | Set CPM to ON
401*1 | Set CPM to OFF
This feature enables or disables CPM. When CPM is off, the unit will disregard ringing, and consider the phone answered. After 5 seconds the notification report will begin.
Units | Default | Min | Max | Options/Comments
N/A | 0 | 0 | 1 | 0=ON,1=OFF

Country Code
402 | Read country code setting
Units | Default | Min | Max | Options/Comments
N/A | N/A | 15 | 22 | 15=KSA, 22=USA

Outgoing Call Timer
403 | Read outgoing call time limit
403** | Reset outgoing call time limit to default
403*V | Set outgoing call answer limit
This is the amount of time that the unit will wait between a destination answering the call, and the start of the session. Associated with Alarmware™, Log File downloading, and Central Station contact.
Units | Default | Min | Max | Options/Comments
SECONDS | 45 | 30 | 120 | N/A

Ring Answer Delay
404 | Read ring answer delay (ring count)
404** | Reset ring answer delay to default
404*V | Set ring answer delay to V
This parameter determines how many rings will be allowed before the unit answers an incoming call.
Units | Default | Min | Max | Options/Comments
RINGS | 1 | 1 | 20 | N/A

Speaker State
405 | Reads speaker state
405** | Reset speaker state to default
405*0 | Set speaker state to ON
405*1 | Set speaker state to OFF
Determines whether or not the speaker is audible during incoming and outgoing over the phone sessions.
Units | Default | Min | Max | Options/Comments
N/A | 0 | 0 | 1 | 0=ON,1=OFF

Call-In Timer
406 | Read Call-in Time Limit
406** | Reset Call-in Time Limit to default
406*V | Set Call-in Time Limit to <V>
This is the amount of time that the unit will wait between answering the call and the start of a session. Associated with Alarmware™, Log File downloading and Central Station contact.
Units | Default | Min | Max | Options/Comments
SECONDS | 60 | 15 | 120 | N/A

Dialing Mode
407 | Read dialing mode
407** | Reset dialing mode to default
407*0 | Set dialing mode to PULSE
407*1 | Set dialing mode to TONE
Units | Default | Min | Max | Options/Comments
N/A | 1 | 0 | 1 | 0=PULSE, 1=TONE

RTU Phone Number
408 | Read RTU Phone Number
408** | Reset RTU Phone Number to NONE
408*DN | Set RTU Phone Number to DN
Units | Default | Min | Max | Options/Comments
N/A | NONE | N/A | N/A |