# Channel Configuration

Keycode | Specification

PIO Channel Configuration
431 | Report the PIO Channel configuration for all points on the IO board.
431** | Reset all PIO Channel configurations on the IO board to default.
431*P | Report the PIO Channel configuration for point Z on the IO board.
431*P** | Reset the PIO Channel configuration for point Z on the IO board to default (DISCRETE).
431*P*0 | Set the PIO Channel configuration for point Z on the IO board to DISCRETE.
431*P*1 | Set the PIO Channel configuration for point Z on the IO board to ANALOG.
Determines how the physical channels are configured. Physical Input channels can be set as either an ANALOG or DISCRETE data type. Analog channel types have a range of values, while discrete channel values are either 1 or 0.

Channel Configuration Report
5 | Review configuration report for all channels
5** | Reset configuration report for all channels
5*Z | Review all configuration data for Channel Z
5*Z** | Reset Channel configuration data.

Channel SNA Configuration
51Z | Read channel Z source net address
51Z** | Reset channel Z source net address
51Z*SNA | Set channel Z source net address

Channel Violation Conditions
52 | Report violation conditions for all channels
52** | Reset violation conditions for all channels
52Z | Review violation conditions for channel Z
52Z** | Reset violation conditions for channel Z
52Z*0 | Disable channel Z
52Z*1 | Set channel Z to Alarm on 1 raw value
52Z*2 | Set channel Z to Alarm on 0 raw value
52Z*3 | Set channel Z to Alarm Never
52Z*4 | Set channel Z Alarm on Com Failure only
52Z*5 | Read low setpoint for channel Z
52Z*5** | Reset low setpoint for channel Z
52Z*5*V | Set low setpoint for channel Z to V
52Z*6 | Read high setpoint for channel Z
52Z*6** | Reset high setpoint for channel Z to default.
52Z*6*V | Set high setpoint for channel Z to V

Transformation Options
53Z | Read transformation option for channel Z
Units | Default | Min | Max | Options/Comments
N/A | RAW | 0 | N/A | 0=RAW

Destination / Channel Groups
Provides operators with the opportunity to determine which channels are linked to which destinations.
55 | Read destination channel groups
55** | Reset all destination channel groups to default
55Z | Read destination channel group for Channel Z.
55Z** | Reset destination channel group for channel Z to default.
Units | Default | Min | Max | Options/Comments
LINKS | ALL | ONE | ALL | N/A

Channel Violation Trip Delay
Determines the amount of time an individual channel can be in a violation condition, before channel goes into an alarm state.
56Z | Read channel Z violation trip delay
56Z** | Reset channel Z violation trip delay
56Z*V | Set channel Z violation trip delay to V seconds
Units | Default | Min | Max | Options/Comments
SECONDS | 2.0 | 0.0 | 9999 | N/A