# List All Active Nodes on Network

This feature reports active nodes found on a specified device.

This report may take a very long time. The Dialer will beep at 5-second intervals while running. You may halt execution at any time by pressing the ENTER key. MODBUS (Also applicable for ModbusTCP and EtherNet/IP) with DEF switch will list all possible nodes. Any Communication alarms that trip during this process will automatically reset when exiting program mode.

Keycode Examples:

To list all active nodes on Network N, press: 914 N ENTER.

Alarmware™ Example:

- To receive a Summary Report for All Network Diagnostic Statistics for a particular network, first connect to the desired RTU.
- Click Diagnostics on the menu bar.
- Select the Net Diagnostics -- Summary Report from the menu items listed.
- Alarmware™ will upload the Net Summary Report to the RTU messages window.