# Data Sampling

This parameter deals with the periodically sampled reading value of channels. This excludes channels that are disabled (inactive), and channels that have been excluded from the Log File or Printer via Destinations Channels Grouping. The intent of this feature is to provide "snapshots" of channel readings at periodic intervals. The base time and frequency parameter determines the data-sampling interval. There are separate sampling intervals for the Log File and Printer devices.