# Panasonic KX-P1180 Printer

This is RACO's standard offering for an off-the-shelf data-logging printer.

The default settings for the printer port, the jumper settings for the KX-PS13 card, and VSER-01 cable are all required for "out-of-the-box" operations.

The jumper settings for the KX-PS13 interface card:

Switch | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
SW1 | OFF | OFF | OFF | OFF | OFF | OFF | ON | ON
SW2 | OFF | ON | OFF | ON | OFF | OFF | ON | OFF

The KX-P11D card does not support DTR flow control and has a small buffer (but switch settings are identical).