# Session and Annunciation Parameters - Keycodes

Keycode | Specification

Callback Settings – Status Report
791 | Read Callback Settings
791** | Clear Callback
791*A | Send Status Report to phone number A in Voice Mode
791D | Send Status Report to destination D
792*A | Send Status Report to phone number A in FAX Mode

Callback Settings – Log File Report
793 | Read Callback Settings
793** | Clear Callback
793*A | Send Log File Report for the last 24 hours to phone number A in FAX Mode
793D | Send Log File Report for the last 24 hours to destination D

Autocall Report
794** | Toggle Autocall Report (enable/disable)

Log File Dump to Printer
799D | Dumps the contents of the log file report to the local printer with the configured parameters for destination D.

Common Trip Delay
801 | Read common trip delay
801** | Reset common trip delay
801*V | Set common trip delay to V seconds
This is the amount of time that a channel violation is allow to exist without the unit changing the channel state to alarm. This setting is common to all channels. Individual channel trip delays should be set after this parameter because changing this parameter changes all channel trip delays to the common trip delay.
Units | Default | Min | Max | Options/Comments
SECONDS | 2.0 | 0.1 | 9999 | N/A

Alarm Reset Time
802 | Read alarm reset time
802** | Reset alarm reset time
802*V | Set alarm reset time to V hours
This setting is the amount of time between alarm acknowledgment, and the unit returning the channel state back to normal.
Units | Default | Min | Max | Options/Comments
HOUR(S) | 1 | 0.1 | 99.9 | N/A

Power Failure Alarm Trip Delay
803 | Read power failure alarm trip delay.
803** | Reset power failure alarm trip delay
803*V | Set power failure alarm trip delay to V minutes
This is the amount of time that the unit will wait before tripping a PFAIL alarm and subsequent notification sequence.
Units | Default | Min | Max | Options/Comments
MINUTE(S) | 1 | 1 | 9999 | 0.0 DISABLES POWER FAILURE ALARM

Phone Fault Test (TFAIL)
804 | Read phone line failure test interval settings
804*0 | Disable phone line failure tests
804*1 | Enable phone line failure tests
804** | Reset phone line failure test settings
When enabled, the unit will test the phone line for dial tone at the interval set by the operator.
Units | Default | Min | Max | Options/Comments
N/A | N/A | N/A | N/A | MUST USE ALARMWARE TO MODIFY THE BASE TIME OR FREQUENCY

Automatic Re-Arm Enable
805 | Report the status of the automatic re-arm feature
805*0 | Disable automatic re-arm feature
805*1 | Enable automatic re-arm feature
805** | Reset automatic re-arm feature to default (disabled)
This parameter will enable the Automatic Re-Arm feature
Units | Default | Min | Max | Options/Comments
N/A | N/A | N/A | N/A |

Automatic Re-Arm Time
806 | Report the status of the automatic re-arm feature
806*V | Set automatic re-arm time to V minutes
806** | Reset automatic re-arm time feature to default
When enabled, this parameter will automatically re-arm the unit after the configured amount of time. This feature is designed to prevent the unit from accidentally being left in a DISARMED state, unable to make outgoing phone calls. Caution is advised however, because this could have unwanted side effects, such as arming the unit when it was should remain disarmed for an extended period of time.
Units | Default | Min | Max | Options/Comments
MINUTES | 60 | 2 | 9999 |

Alarm Acknowledgment Options
813 | Read acknowledgment option
813** | Reset acknowledgment option to default
813*1 | Set acknowledgment option to OFF
813*2 | Set acknowledgment option to PIN required
This setting determines how incoming calls to the unit are handled when an alarm condition exists. Alarms can be automatically acknowledged when a PIN is entered.
Units | Default | Min | Max | Options/Comments
N/A | 1 | 0 | 2 | 1=OFF, 2=REQUIRE PIN

Inter-session Delay
820 | Read inter-session delay value
820** | Reset inter-session delay value to default
820*V | Set inter-session delay to V minute
This is the period of time between outgoing phone calls. Intent is to provide an opportunity for operators to call the unit.
Units | Default | Min | Max | Options/Comments
MINUTES | 0.5 | 0.0 | 60.0 | N/A

Redial Attempts to the Same Destination
823 | Read redial attempts
823** | Reset redial attempts to default
823*V | Set redial attempts to V
This parameter determines how many times a particular destination will be consecutively contacted. Destination may be called again if no destination has acknowledged the alarms and the unit is forced to loop back to the first eligible destination.
Units | Default | Min | Max | Options/Comments
ATTEMPTS | 1 | 1 | 5 | N/A

Session Time-Out
824 | Read session time-out value
824** | Reset session time-out to default
824*V | Set session time-out to V seconds
This parameter defines how long the RTU can be inactive, before a session is terminated. Purpose is to ensure the unit is not left in program mode for extended periods of time.
Units | Default | Min | Max | Options/Comments
SECONDS | 60 | 0.1 | 3600 | N/A

Listening Period Options
825 | Read end of session listening period option
825** | Reset end of session listening period option to default
825*0 | Set end of session listening period option to ON
825*1 | Set end of session listening period option to OFF
Listening period when enabled will add 15 seconds to the end of an over the phone session, to allow operators to listen to the ambient noise surrounding the unit. Menu options are available during the listening period.
Units | Default | Min | Max | Options/Comments
N/A | 1 | 0 | 1 | 0=ON,1=OFF

Menu Options Repeat
826 | Read current Option Menu Prompt Repeat value
826** | Reset Option Menu Prompt Repeat to default
826*V | Set Option Menu Prompt Repeat to value
The Menu Options Repeat parameter determines whether or not the menu options are to be repeated during an over the phone session with a RTU. Administrators may decide that the menu options should not be repeated at all for security reasons. Others may deem that the unit should repeat the menu more than once for novice operators. This feature provides administrators a greater flexibility.
Units | Default | Min | Max | Options/Comments
REPEATS | 0 | 0 | 3 | N/A

Protocol Detection for Incoming Calls
827 | Reports current protocol detection time limit
827** | Resets current protocol detection time limit to default
827*V | Set current protocol detection time limit to V seconds
Units | Default | Min | Max | Options/Comments
SECONDS | 7 | 3 | 60 | N/A