# Report All Network Diagnostic Statistics for All Networks

This function will report all the diagnostic information for all networks.

Diagnostic information includes:

Configuration Summary for Modbus Network:

Scan is ENABLED.

Protocol is MBMASTER.

Local node address is 1.

Communications alarm timer is 200 second(s).

Transaction timer is 0.2 second(s).

Delay timer is 0 second(s).

Serial parameters for device 1:

Stopbits are 1.

Databits are 8.

Baudrate is 9600.

Parity is EVEN.

Configuration Summary for Ethernet Network:

Scan is ENABLED.

Protocol is Ethernet.

Local node address is 1.

PLC Communications Report for NET 1:

Scan time is 0 second(s).

Communication with all node(s) is normal.

The total error count is 0.

Last 10 errors are: 0, 0, 0, 0, 0, 0, 0, 0, 0, 0

Alert count is 0.

Configuration Summary for Printer:

Scan is ENABLED.

Language is ENGLISH.

Report format is all text.

Linked to channels: 1-10, 101-256.

Conditions logged are: session attempts, configuration changes, channel alarms, acknowledgment and reset-to-normal.

Serial parameters for device 2:

Stopbits are 1.

Databits are 8.

Baudrate is 19200.

Parity is NONE.

Flow control option is RTS/CTS/DTR.

Configuration Summary for AlarmWare Port:

Protocol is SFP.

Serial parameters for device 3:

Stopbits are 1.

Databits are 8.

Baudrate is 57600.

Parity is NONE.

Configuration Summary for Log File:

Scan is ENABLED.

Language is ENGLISH.

Linked to channels: 1-90, 111-200, 211-256.

Conditions logged are: ALL.

Data sampling is ENABLED:

start DAILY at 00:00 (HH:MM)

repeat interval is 00:00:05:00 (DD:HH:MM:SS).

Data sampling parameters are:

800 Kbytes reserved for log file.

Auto-start logfile session is at 90 percent of limit.

Logfile overflow option is STOP LOGGING.

Keycode Examples:

- To receive a report for all network diagnostic statistics for all networks, press: 902 ENTER.
- To reset all network diagnostic statistics for all networks, press: 902 ** ENTER.

Alarmware™ Example:

- To receive a Summary Report for All Network Diagnostic Statistics for a particular network, first connect to the desired Catalyst.
- Click Diagnostics on the menu bar.
- Select the Net Diagnostics -- Summary Report menu item.
- Alarmware™ will upload the Net Summary Report to the RTU messages window.