# Alarmware Port

To make changes to the Alarmware™ Port settings (the network used to establish serial port connection with a computer running Alarmware™ locally at the RTU) either connect or work off-line with desired RTU. Select Devices from the Configuration menu. In the tabbed dialog box labeled "Device Settings" select the Alarmware Port tab:

Note: Only the Baud Rate may be altered in this version of Alarmware™ or the RTU.

Baud Rate -- Select desired Baud Rate from list. The Baud Rate value must match the Baud Rate configured for the COM port used by the Alarmware Host computer, as shown below: