# Flash Memory Module Installation Procedure

To install additional NVRAM on the Catalyst, please adhere to the following procedure:

1. Start by saving your configuration to Alarmware™. Connect Alarmware™ to the proper Catalyst and import the configuration. Quit the session after import completed.
2. Next, press the "Power Off" key on the front panel of the Catalyst.
3. Remove power from the Catalyst by disconnecting the battery, then unplugging the main power cord from its power source.
4. Open the Catalyst cover.
5. Find the two PCB standoffs provided and install them on the "System PCB" as shown in Diagram 2.15. The collared end of the support should be facing down. Press down on the supports until they snap into place.
6. Next take the flash memory board and line it up with the connector. Make certain that all pins are lined up correctly and press down until completely seated.
7. Install the support screws and tighten.
8. Reconnect the battery.
9. Close the Catalysts cover and reconnect the power source.
10. The Catalyst will automatically cycle Power ON, then will automatically reformat the file system.
11. Reconnect with Alarmware and export the saved configuration from Alarmware back to the Catalyst.

Diagram 2.15