# Destination Number

Each Destination is assigned an ordinal number by which it is known. Enter the number of the Destination you wish to configure in the designated field. Your choices for destination number have a functional importance, in that when a single channel goes into Unacknowledged Alarm State, it will issue reports to the available destinations to which it is linked, in priority based upon lowest ordinal Destination number first.

Exception: power failure alarms will result in calling all voice mode (personnel) phone number destinations, with priority based upon lowest Destination number first.

In the special situation where there are two or more channels in Unacknowledged Alarms state simultaneously, alarm reports will be issued in priority either according to lowest ordinal Destination number, or else according to lowest ordinal channel number, depending upon which mode is selected in the Session Parameters dialog box.