# Alarm Notification

This type of session deals with current UNACKNOWLEDGED ALARM conditions. The report only includes channels linked in the destination's group. The intent of this report is to obtain operator acknowledgment. These reports are scheduled as the alarm states arise. Details of alarm notification sessions depend on destination type, annunciation sequence, and session parameter configurations.