# Time to complete a Scan for the Channels using Network

This feature reports the time required making a complete scan of all the channels for a particular network. A channel not in communication alarm is guaranteed to have latency less than the scan time. If in communication alarm, latency is greater than the Communication Alarm Trip Delay Timer value for that net.

Keycode Examples:

- To receive a report for all network diagnostic statistics for all networks, press: 902 ENTER.

Alarmware™ Example:

- To receive a Summary Report for All Network Diagnostic Statistics for a particular network, first connect to the desired RTU.
- Click Diagnostics on the menu bar.
- Select the Net Diagnostics -- Summary Report menu item.
- Alarmware™ will upload the Net Summary Report to the RTU messages window.