This tool will help you:

1. -- Determine the appropriate size for your Log File Reserve. The 
amount of memory to reserve is based upon the following factors:

---- a. The amount of installed non-volatile memory (your Catalyst has been 
	shipped to you with 1 to 5 Megabytes of "non-volatile" 
	memory depending on amount ordered from the factory)
---- b. The number of channels to be sampled and stored in the log file
---- c. How often the channels are to be sampled
---- d. How often the Log File data is downloaded to a permanent storage device

2. -- Plan for user-recorded messages. This tool will help you plan how the 
channel speech and text messages can be recorded. You can time each message 
while reciting them. Totals are accumulated to show how much recording time 
remains. Message timing can be repeated as often as necessary. The total 
recording time available can be doubled by selecting the slower recording rate.

3. -- Walk through setting up the channels to be sampled as well as how the 
various destinations will be configured.

4. -- Save and Print the data to refer to when configuring your Catalyst with
keycodes or with the Alarmware software shipped to you with your Catalyst.

To begin, click Start.