# Log File Event Examples

The following are examples of logged events:

RTU Events

Session History

Fri May 18, 2001 11:42:22 Starting session with Central Computer.

Fri May 18, 2001 11:42:22 Alarmware request.

Wed May 16, 2001 11:01:42 The current date is set to 5/18/01, Friday.

The current time is set to 11:42:24.

Fri May 18, 2001 11:39:40 Alarmware session concluded: Alarmware operator requests disconnection.

Fri May 18, 2001 11:39:52 Answering incoming call.

Fri May 18, 2001 11:39:58 Starting voice mode session.

Configuration Changes

Modbus Network Communications alarm timer is set to 30 second(s)

Inter-call delay is set to 1 minute(s).

Alarm Reset time is set to 0.1 hour(s).

Phone line failure tests are DISABLED.

Data Samples

Fri May 18, 2001 12:00:00 Channel Data Sample:

Chamber Temperature is 250 degrees NORMAL

Generator Voltage is 108 volts NORMAL

Liquid Nitrogen level is 713 feet NORMAL

Helium Tank level is 877 gallons NORMAL

Engine Oil Pressure is 250 psi NORMAL

Circulating Pump #14 running NORMAL

Broiler Temperature is 426 degrees HIGH SETPOINT ALARM

Channel Events

Alarms

Fri May 18, 2001 11:40:34 Circulating Pump #14 is not running ALARM

Fri May 18, 2001 12:00:00 Broiler Temperature is 426 degrees HIGH SETPOINT ALARM

Alarm Acknowledgment

Fri May 18, 2001 11:41:52 Reported alarms are acknowledged.

Fri May 18, 2001 11:41:52 Circulating Pump #14 is not running ALARM, ACKNOWLEDGED

Channel Reset to Normal

Fri May 18, 2001 11:42:24 Circulating Pump #14 is not running ALARM, ACKNOWLEDGED NOW NORMAL

Fri May 18, 2001 11:42:36 Circulating Pump #14 running NORMAL