# Messages and Tag Words

Keycode | Specification

RTU Name Message
60 | Listen to RTU Name message
60* | Record RTU Name message
60** | Erase RTU Name message to default

Network ID Messages
61 | Listen to all active network ID messages
61** | Reset Network ID messages to default.
61N | Listen to network N ID message
61N* | Record network N ID message
61N** | Erase network N ID message
Units | Default | Min | Max | Options/Comments
N/A | N/A | 1 | 4 | N/A

Destination ID Messages
62** | Reset all destination messages to default.
62N | Listen to destination N ID message
62N* | Record destination N ID message
62N** | Erase destination N ID message

Tag Words
These words define different channel states. Operators have the flexibility to change the factory words to user-recorded tag words.
64** | Reset All Tag Words to default
641 | Listen to alarm state tag “Normal”
642 | Listen to alarm state tag “Alarm”
643 | Listen to alarm state tag “Alarm Acknowledged”
644 | Listen to alarm state tag “Now Normal”
645 | Listen to alarm state tag “Now Normal, Acknowledged”
647 | Listen to alarm state tag “Alert”
648 | Listen to alarm state tag “High Setpoint”
649 | Listen to alarm state tag “Low Setpoint”
6410 | Listen to alarm state tag “DNA”
6411 | Listen to alarm state tag “SNA”
6412 | Listen to alarm state tag “Status Only”
64N* | Record alarm state tag N
64N** | Erase alarm state tag N and restore default.
Units | Default | Min | Max | Options/Comments
N/A | N/A | 1 | 12 | TAG WORD N

Autocall Message
This feature allows you to record a special message to be played during a scheduled test call
65 | Review Autocall Message
65* | Record Autocall Message
65** | Erase Autocall Message (Voice Only)

Message Time
This is the amount of time available for recording speech messages at the current recording rate.
690 | Report message time available

Recording Rate
693 | Read recording rate
693** | Reset recording rate to default.
693*1800 | Set recording quality to 1800 BPS
693*3600 | Set recording rate to 3600
Units | Default | Min | Max | Options/Comments
BPS | 3600 | 1800 | 3600 | N/A