# Tag Words for Analog Channels

Analog Message = Preamble (Message 1) + Analog Reading + Epilogue (Message 2)

Channel State |  | No Current Violation Exists
NORMAL |  | Analog Message + "Normal"
UNACKNOWLEDGED ALARM |  | Analog Message + "Alarm, Now Normal"
ACKNOWLEDGED ALARM |  | Analog Message + "Alarm, Acknowledged, Now Normal"

Channel State |  | Current Violation Exists
ALERT |  | Analog Message + "Alert"
UNACKNOWLEDGED ALARM |  | Analog Message + "Alarm"
ACKNOWLEDGED ALARM |  | Analog Message + "Alarm, Acknowledged"