# Voice Mode Tag Words - Keycodes

You may record your own voice mode Tag Words to replace the factory default ones. To have an adequate understanding of Tag Words, please refer to Tag Words and States.

The Keycodes for reading the Tag Words based upon the factory defaults are:

Keycode | Tag Words
--- | ---
6 4 1 | NORMAL
6 4 2 | ALARM
6 4 3 | ALARM ACKNOWLEDGED
6 4 4 | NOW NORMAL
6 4 5 | NOW NORMAL ACKNOWLEDGED
6 4 7 | ALERT
6 4 8 | HIGH SET POINT
6 4 9 | LOW SET POINT
6 4 10 | DNA COMMUNICATIONS
6 4 11 | SNA COMMUNICATIONS
6 4 12 | STATUS ONLY
To record your own replacement tags, add * after the above digits. To restore tags to default, add * * after the above digits.