# Channel Status, Value, and State Reports

Keycode | Specification

Status Reports
0 | Channel status summary report
00 | Review full status report
00Z | Read status of channel Z

Channel Value Reports
01 | Current value of all channels
01*SNA | Read current value at net address
01*SNA*V | Write value to net address
01Z | Read current value of channel Z
01Z*V | Write value to channel Z
01ZZ** | Channel value reset without write-back
Units | Default | Min | Max | Options/Comments
n/a | n/a | n/a | n/a | n/a

Communications Status Reports
02 | Review full communications status report
02Z | Report communications status for channel Z

Channel Raw Value Reports
03Z | Report default (raw) value for channel Z

Channel State Summary Reports
05 | Channel state summary report