# Items to be reported to This Destination

You can filter the log file data that is delivered to a particular destination. If a destination type is eligible to receive log file reports, you have the following options available:

RTU Events:

- Data Samples - includes snapshots of channel values and states
- Session History – includes all session-related messages
- Configuration Changes - includes all RTU configuration changes

Channel State Transitions:

- Alarms - includes all channel alarm data
- Alarm Acknowledgment - includes messages pertaining to when an alarm is acknowledged
- Reset – includes messages logged when channels are reset to normal

Include Log File Data in the following range:

- All Data - includes all channel alarm data and notification reports
- Undelivered Data Only - include only data that has not been delivered to this destination
- Data Collected in the Previous DD:HH – include data logged during the previous day:hour