# Voice Mode Destination ID Name Messages

Voice Mode Destination ID Messages are most commonly used in text reports or logs, to identify personnel at the telephone numbers where they will be receiving alarm calls. Typically, user recorded Voice Mode Destination ID messages are the names of the corresponding individuals. If more than one person might be reached at a given telephone number configuring PINs provides a way to more reliably identify the exact individual who receives an alarm call in text logs and reports. Regardless, Voice Mode Destination ID voice messages will be encountered much less frequently than their text counterparts. The factory default Voice Mode Destination ID Name message for Destination N is "Destination N".

Keycodes:

- To review the Voice Mode Destination N ID message use Keycode 6 2 N
- To clear the Voice Mode Destination N ID message to factory default use Keycode 6 2 N * *
- To record the Voice Mode Destination N ID message use Keycode 6 2 N *