# Diagnostic Codes for the Last Ten Network Problems

This function reports on the last 10 communication errors for a specified device. These are errors only. It is not necessary for them to have tripped a communication alarm violation.

Note: No time information provided. Any error mentioned may have been repeated any number of times.

Keycode Examples:

To receive a report for the Last Ten Network Problems, enter keycode: 902N4 ENTER.

Alarmware™ Example:

1. To receive a Summary Report for All Network Diagnostic Statistics for a particular network, first connect to the desired RTU.
2. Click Diagnostics on the menu bar.
3. Select the Net Diagnostics -- Summary Report.
4. Alarmware™ will upload the Net Summary Report to the RTU messages window.