# Speaker Enable

This function controls the state of the RTU local speaker during remote voice sessions. If selected ON, both sides of a voice session between the RTU and a remote user will be heard through the speaker. If selected OFF, the RTU will be silent during remote voice session. The speaker is always ON when a Front Panel session is in progress, regardless of this parameter. The default is ON