# Voice Mode RTU Name Messages

The Voice Mode RTU Name Message is used to identify the site where the RTU is located. An example for this message might be, "This is the South Main Pumping Station." This message will be the first message heard when calling the RTU or receiving alarm reports in voice mode. Using the leading words "This is…" will usually be helpful in making the nature of the call more clear to the recipient. The factory default Voice Mode RTU Name Message is "RTU."

Important Note: If the RTU Name message is very long, the timing of data connections can be affected. The amount of time it takes to connect with Alarmware™ and other devices is increased by the length of time it takes to recite the message. It may become necessary to extend the call-in timer or shorten the message.

Keycodes:

- To review the Voice Mode RTU name message use Keycode 6 0
- To clear the Voice Mode RTU name message to factory default use Keycode 6 0* *
- To record the Voice Mode RTU name message use Keycode 6 0 *